**Instructions to update the BIOS for NEO Z100-0dB.**

1. Boot the NEO Z100-0dB and the Windows OS.

2. Under Windows OS, extract the BIOS files and copy them to a random folder.

3. Right-click the 'FlashBIOS.bat' file, choose 'Run as Administrator'.



4. The BIOS will be updated automatically.

5. When it's done, restart the device.

Please note, it takes more time than usual for the device to boot up, as it's the first time of booting up after updating the BIOS.

**Note: 1. Please put the bios in the root directory**

**2. Please stop flash bios and contact us if there any error happening during process.**

**3.It is with risk when flash bios firmware,it is not recommended to flash bios if there is no necessarily necessary.**

**4.Please make sure the power adapter is connecting while flash the bios,once the power lost the device is dead.**